High performance double inlet centrifugal fans with forward curved blades.
Volume flow from 200 m3/h to 140.000 m3/h
Total pressure up to 2.000 Pa.
Sizes from 160 up to 1.000,
with scaling in accordance to AMCA Standard 99-0098 76 R20 and to DIN 323 R20.
