Version supported on strong rectangular side frames, made of galvanised steel, welded on the scroll sides.  Ball bearings on cast iron pillow blocks with grease points.  
Available from the size 20-15 up to the size 30-28.
The standard fan can be freely rotated, to allow installation with orientation 0°, 90°, 180° or 270°, as defined in ISO 13349.
