High performance double inlet centrifugal fans with airfoil blades.
Volume flow from 2000 m3/h to 150.000 m3/h
Total pressure up to 3.000 Pa.
Sizes from 315 up to 1000,
with scaling in accordance to AMCA Standard 99-0098 76 R20 and to DIN 323 R20.
