Version supported on strong rectangular side frames, made of galvanised steel, welded on the scroll sides.  Ball bearings on cast iron pillow blocks with grease points.  
Available from the size 9-7 up to the size 18-18.
The standard fan can be freely rotated, to allow installation with orientation 0°, 90°, 180° or 270°, as defined in ISO 13349.
