High performance double inlet centrifugal fans with backward inclined blades.
Volume flow from 200 m3/h to 250.000 m3/h
Total pressure up to 3.500 Pa.
Sizes from 180 up to 1400,
with scaling in accordance to AMCA Standard 99-0098 76 R20 and to DIN 323 R20.
